**Disconnect Sensor**

* **Actor**– Pusher
* **Preconditions**– At least one sensor is connected and assigned to a channel
* **Normal course** – The sensor is disconnected from previously-assigned channel
* **Alternate courses** –
* **Exception courses** –
* **Post-conditions** – One less sensor is connected, and one channel is now live but unassigned to a sensor
* **Frequency of use** – 4x/day of events
* **Assumptions**–